**Personnel:**

Stergious Aji

Hang Dai

Chaitanya Kaul

**Depth Cameras:**

All cameras use SWIR (~800-900nm) class 1 laser/LED illumination for depth capture

|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Specification** | **Depth?** | **RGB (webcam)?** |
| Intel | L515 | Yes | Yes |

**Radar Transceivers**

|  |  |  |
| --- | --- | --- |
| **Company** | **Specification** | **Radiofrequency (GHz)** |
| Google | SOLI (ATAP) | 60 |

**Devices:**

TBD: Show Pictures